

Glanmire window surround guide (Stick on)

15/11/2019

|  |  |  |  |
| --- | --- | --- | --- |
| Brick ope | External | Internal | Clear ope |
| 648 | 828 | 628 | 548 |
| 872 | 1052 | 852 | 772 |
| 1435 | 1615 | 1415 | 1335 |
| 1660 | 1840 | 1640 | 1560 |
| 1885 | 2065 | 1865 | 1785 |
| 2110 | 2290 | 2090 | 2010 |

All dimensions are in millimetre. For internal lengths greater than 2090mm the head units are divided and require structural support.